**Supplies needed**

* Two 13” by 18” (inch) pieces of printed cotton material for OUTSIDE bag
* Two 13” by 18” (inch) pieces of plain cotton material for LINING of bag
* 4 meters of cording

**Fabric KEY Symbol KEY**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OUTSIDE MATERIAL | LINING MATERIAL |  | Dots | Stitching line | C:\Users\15261\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\50I6B38W\yzEgW[1].pngMulti zigzag |

**Seam allowance -** 1.5cm unless otherwise stated

**Instructions**

|  |  |
| --- | --- |
| * Pin one OUTSIDE piece to one LINING piece with WRONG sides together * **Multi Zigzag** (3,D,1.5) so the zigzag is as close to the edge fabric as possible. * ***Repeat*** for other outside and lining material | C:\Users\15261\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\50I6B38W\yzEgW[1].png  Multi Zigzag  C:\Users\15261\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\50I6B38W\yzEgW[1].pngC:\Users\15261\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\50I6B38W\yzEgW[1].png  x  C:\Users\15261\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\50I6B38W\yzEgW[1].pngC:\Users\15261\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\50I6B38W\yzEgW[1].pngC:\Users\15261\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\50I6B38W\yzEgW[1].pngC:\Users\15261\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\50I6B38W\yzEgW[1].pngC:\Users\15261\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\50I6B38W\yzEgW[1].png |
| * With OUTSIDE material right sides together pin the two long sides and the bottom together. * From the top of your bag **mark 1st dot 5 cm down and the 2nd dot 7 cm down**. * Sew starting at the top with a regular straight stitch around the bag – **DO NOT SEW BETWEEN THE TWO DOTS.** * Backstitch at beginning and end, as well as by the dots |  |
| * Fold the top of bag towards the LINING side 4 cm * Top stitch all the way around by lining up the folded edge with the edge of the throat plate of your machine * Make sure you DO NOT sew over your holes |  |
| * Cut cord into two equal lengths 2 meters each * Starting at one hole thread the 1st cord all the way back to where you started. Leave the cord long * Repeat at the other hole - thread the 2nd cord all the way back to where you started. Leave the cord long |  |
| * Now you are ready to insert the two grommets at the bottom corners of your bag. ***Need to go to computer room 203*** * Thread cord through grommet and tie a knot to secure |  |